Capsule API Example

Loading...
Searching...
No Matches
Devices Modes

# Impedance measurement

## Methods:

- clCResistance_GetCount - the number of channels
- clCResistance_GetChannelName - the name of a channel
- clCResistance_GetValue - the resistance of a channel

The resistance value for each channel, in order to receive good signal, it is recommended to be lowered according to the following estimate:

- Above 1000 kOhm - bad quality
- 500 to 1000 kOhm - average quality
- Below 500 kOhm - good quality

## Get channel info:

You can use these methods any time after creating the device.

- clCDevice_GetChannelNames
- clCDevice_ChannelNames_GetChannelsCount
- clCDevice_ChannelNames_GetChannelIndexByName
- clCDevice_ChannelNames_GetChannelNameByIndex

## Device mode events:

- clCDevice_SetOnModeSwitchedEvent

In signal mode received EEG data already free of miographic artifacts. If artifacts detected, invalid values are not sent via API.