Capsule API Example

Loading...
Searching...
No Matches
clCNFB

To get [Timestamp, Delta, Theta, Alpha, SMR, Beta] a callback is used with a pointer to `clCNFB_UserState`, which is set via clCNFB_SetOnUserStateChangedEvent

## Call Result values:

- 0 - Success
- 1 - FailedToSendData

## Methods:

- clCNFB_Create
- clCNFB_CreateCalibrated

## NFB events:

- clCNFB_SetOnUserStateChangedEvent
- clCNFB_SetOnErrorEvent

You can receive values of the following main brain rhythms without calibration: Theta (4-7 Hz), Alpha (7-13 Hz), Beta (15-30 Hz). All values are sent in mV^2.

Method `clCNFB_CreateCalibrated` allows you to create a classifier after calibration individual nfb data